Welcome Dear Customer!!!
If you are reading this document then you have succeeded in downloading your first updates from our server.

JTAG Manager software for RIFF BOX will allow you:
•	Resurrect many firmware killed devices which have no ROM bootcore code or bootstrap ability but have hardware JTAG interface enabled;
•	Perform simple JTAG related operations like halting core, restarting core, running core, reading and writing core’s memory, etc;
•	Due to DCC Loader feature you can access complicated peripherals like NAND memory, perform reads and writes in all existent NAND memory modes;
•	Develop your own hardware scripts in order to communicate with yet not supported hardware chipsets (chipsets, not cores);

Please do not forget to check frequently if new updates are available and download them in order to keep as up-to-date as possible.

Enjoy using our RIFF BOX software products!!!